From 198bd175e3dea90041b1e183d5b337dc26d0e848 Mon Sep 17 00:00:00 2001
From: Trygve Laugstøl <trygvis@inamo.no>
Date: Fri, 27 Apr 2018 02:17:52 +0200
Subject: wip

---
 slides/images/IP-Header_eng.tex | 47 -----------------------------------------
 1 file changed, 47 deletions(-)
 delete mode 100644 slides/images/IP-Header_eng.tex

(limited to 'slides/images/IP-Header_eng.tex')

diff --git a/slides/images/IP-Header_eng.tex b/slides/images/IP-Header_eng.tex
deleted file mode 100644
index 8de7312..0000000
--- a/slides/images/IP-Header_eng.tex
+++ /dev/null
@@ -1,47 +0,0 @@
-\iffalse
-Lorem Ipsum is simply dummy text of the printing and typesetting industry. Lorem Ipsum has been the industry's standard dummy text ever since the 1500s, when an unknown printer took a galley of type and scrambled it to make a type specimen book. It has survived not only five centuries, but also the leap into electronic typesetting, remaining essentially unchanged. It was popularised in the 1960s with the release of Letraset sheets containing Lorem Ipsum passages, and more recently with desktop publishing software like Aldus PageMaker including versions of Lorem Ipsum.
-\fi
-
-\begin{tikzpicture}[scale=0.30]
-	\sffamily
-	\foreach \x in {0,7,8,15,16,31} % {0,...,32}
-		\node at (\x+0.5,20.5) {\scriptsize \x};
-%	\foreach \x in {0,...,31}
-%		\node at (\x+0.5,13.5) {\scriptsize \x};
-	\foreach \x in {0,8,16,32} % {0,...,32}
-		\draw[thick] (\x,20) -- (\x,21);
-	\foreach \x in {0,...,32}
-		\draw[thick] (\x,14) -- (\x,20);
-%	\foreach \x in {0,...,32}
-%		\draw[thick] (\x,13) -- (\x,14);
-	\node[thick] (bit1) at (-0.6,20.5) {\scriptsize bit};
-%	\node[thick] (bit2) at (-0.6,13.5) {\scriptsize bit};
-		
-\iffalse
-	\draw [<->, thick] (-0.6, 19.9) -- (-0.6,15.1);
-	\draw [thick] (-1, 20) -- (-0.1,20);
-	\draw [thick] (-1, 15) -- (-0.1,15);
-	\node[fill=white] at (-1.1,17.5) {\tiny 20 bytes};
-\fi
-	\foreach \y/\v in {0,4,8,12,16,20}
-		\node at (-0.6,{19.5-(\v / 4)}) {\scriptsize \v};
-
-	\filldraw[thick,draw=black, fill=white] (0,20) rectangle (4,19); \node (mode) at (2,19.5) {\scriptsize version};
-	\filldraw[thick,draw=black, fill=white] (4,20) rectangle (8,19); \node (mode) at (6,19.5) {\scriptsize len};
-%	\draw[thick, draw=black, fill=white] (8,20) rectangle (16,19); \node (stratum) at (11.5,19.5) {\scriptsize type of service (TOS)};
-	\draw[thick, draw=black, fill=white] (8,20) rectangle (16,19); \node (stratum) at (11.5,19.5) {\scriptsize TOS};
-	\draw[thick, draw=black, fill=white] (16,20) rectangle (32,19); \node (li) at (24,19.5) {\scriptsize full length of packet};
-	\filldraw[thick,draw=black, fill=white] (0,19) rectangle (16,18); \node (mode) at (8,18.5) {\scriptsize identification};
-%	\draw[thick, draw=black] (16,19) rectangle (19,18); \filldraw[white] (16.5,18.43) rectangle (19,18.88); \node [](li) at (17.5,18.67) {\tiny IP flags}; \node at (16.5,18.25) {\tiny x};\node at (17.5,18.25) {\tiny D};\node at (18.5,18.25) {\tiny M};
-	\draw[thick, draw=black] (16,19) rectangle (19,18); \filldraw[white] (16.5,18.43) rectangle (19,18.88); \node at (16.5,18.5) {\scriptsize X};\node at (17.5,18.5) {\scriptsize D};\node at (18.5,18.5) {\scriptsize M};
-	\draw[thick, draw=black, fill=white] (19,19) rectangle (32,18); \node (li) at (24,18.5) {\scriptsize fragment Offset};
-	\filldraw[thick,draw=black, fill=white] (0,18) rectangle (8,17); \node (mode) at (4,17.5) {\scriptsize time to live (TTL)};
-	\draw[thick, draw=black, fill=white] (8,18) rectangle (16,17); \node (stratum) at (11.5,17.5) {\scriptsize protocol};
-	\draw[thick, draw=black, fill=white] (16,18) rectangle (32,17); \node (li) at (24,17.5) {\scriptsize header checksum};
-	\filldraw[thick,draw=black, fill=white] (0,17) rectangle (32,16); \node (mode) at (16,16.5) {\scriptsize source IP address};
-	\filldraw[thick,draw=black, fill=white] (0,16) rectangle (32,15); \node (mode) at (16,15.5) {\scriptsize destination IP address};
-	\draw[thick,draw=black, fill=white] (0,15) rectangle (31.5,14);
-	\draw[fill=white, draw=white] (31.4,14.96) rectangle (31.6,14.05);
-	\draw[thick]  (31.5,14.97)  decorate [decoration=saw] { -- (31.5,14.02)};
-	\node (mode) at (16,14.5) {\scriptsize IP options (variable length)};
-\end{tikzpicture}
-- 
cgit v1.2.3

